CHIPname=10F200
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000100
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=10F202
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=10F204
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000100
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=10F206
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=10F220
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000100
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=10F222
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=NewF12B
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FEF

CHIPname=12C508
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12C508A
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12C509
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12C509A
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12F509
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=6
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=20
ProgramFlag2=1
PanelSizing=0
CoreType=newf12b
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12CE518
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12CE519
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=02
CoreType=bit12_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FFB
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FEF
LIST3 FUSE1 "Oscillator" "EX_RC"=0FFF "IN_RC"=0FFE "XT"=0FFD "LP"=0FFC
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=0FF7

CHIPname=12C671
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3F7F
LIST3 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST4 FUSE1 "Oscillator" "EXRCCK"=3FFF "EXRC"=3FFE "INRCCK"=3FFD "INRC"=3FFC "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2ADF "CP75"=15BF "ALL"=009F

CHIPname=12C672
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=0520
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3F7F
LIST3 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST4 FUSE1 "Oscillator" "EXRCCK"=3FFF "EXRC"=3FFE "INRCCK"=3FFD "INRC"=3FFC "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2ADF "CP75"=15BF "ALL"=009F

CHIPname=12CE673
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3F7F
LIST3 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST4 FUSE1 "Oscillator" "EXRCCK"=3FFF "EXRC"=3FFE "INRCCK"=3FFD "INRC"=3FFC "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2ADF "CP75"=15BF "ALL"=009F

CHIPname=12CE674
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=Y
BandGap=N
ICSPonly=N
ChipID=0520
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3F7F
LIST3 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST4 FUSE1 "Oscillator" "EXRCCK"=3FFF "EXRC"=3FFE "INRCCK"=3FFD "INRC"=3FFC "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2ADF "CP75"=15BF "ALL"=009F

CHIPname=12F629
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=31FF
CPwarn=N
CALword=Y
BandGap=Y
ICSPonly=N
ChipID=0F80
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Bandgap" "Highest"=3FFF "Mid High"=2FFF  "Mid Low"=1FFF "Lowest"=0FFF
LIST8 FUSE1 "Oscillator" "RC CLKGP4 RCGP5"=3FFF "RC IOGP4 RCGP5"=3FFE "INTOSC CLKGP4 IOGP5"=3FFD "INTOSC IOGP4 IOGP5"=3FFC "EC IOGP4 CLKINGP5"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=12F675
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=31FF
CPwarn=N
CALword=Y
BandGap=Y
ICSPonly=N
ChipID=0FC0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Bandgap" "Highest"=3FFF "Mid High"=2FFF  "Mid Low"=1FFF "Lowest"=0FFF
LIST8 FUSE1 "Oscillator" "RC CLKGP4 RCGP5"=3FFF "RC IOGP4 RCGP5"=3FFE "INTOSC CLKGP4 IOGP5"=3FFD "INTOSC IOGP4 IOGP5"=3FFC "EC IOGP4 CLKINGP5"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=12F683
INCLUDE=Y
KITSRUS.COM=8pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=00800
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0460
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16C505
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=8
PanelSizing=01
CoreType=bit12_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=0FFF "Disabled"=0FF7
LIST2 FUSE1 "MCLRE" "Enabled"=0FFF "Disabled"=0FDF
LIST3 FUSE1 "Oscillator" "EXRCCLK"=0FFF "EXRCRB4"=0FFE "INRCCLK"=0FFD "INRCRB4"=0FFC "HS"=0FFA "XT"=0FF9 "LP"=0FF8
LIST4 FUSE1 "Code Protect" "Disabled"=0FFF "Enabled"=002F

CHIPname=16C554
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=00CF

CHIPname=16C558
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=00CF

CHIPname=16C61
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Enabled"=3FFF "Disabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16C62
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FBF "Disabled"=3FBB
LIST2 FUSE1 "PWRTE" "Enabled"=3FBF "Disabled"=3FB7
LIST3 FUSE1 "Oscillator" "RC"=3FBF "HS"=3FBE "XT"=3FBD "LP"=3FBC
LIST4 FUSE1 "Code Protect" "Disabled"=3FBF "CP50"=3FAF "CP75"=3F9F "ALL"=3F8F

CHIPname=16C62A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C62B
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C63
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C63A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C64
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C64A
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C65
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FBF "Disabled"=3FBB
LIST2 FUSE1 "PWRTE" "Enabled"=3FBF "Disabled"=3FB7
LIST3 FUSE1 "Oscillator" "RC"=3FBF "HS"=3FBE "XT"=3FBD "LP"=3FBC
LIST4 FUSE1 "Code Protect" "Disabled"=3FBF "CP50"=3FAF "CP75"=3F9F "ALL"=3F8F

CHIPname=16C65A
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C65B
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C66
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=0380
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C67
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C620
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=35DF

CHIPname=16C620A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=35DF

CHIPname=16C621
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=35DF

CHIPname=16C621A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=35DF

CHIPname=16C622
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C622A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C71
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Enabled"=3FFF "Disabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16C71A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FF7
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=004F

CHIPname=16C72
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C72A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C73
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FBF "Disabled"=3FBB
LIST2 FUSE1 "PWRTE" "Enabled"=3FBF "Disabled"=3FB7
LIST3 FUSE1 "Oscillator" "RC"=3FBF "HS"=3FBE "XT"=3FBD "LP"=3FBC
LIST4 FUSE1 "Code Protect" "Disabled"=3FBF "CP50"=3FAF "CP75"=3F9F "ALL"=3F8F

CHIPname=16C73A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C73B
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FBF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C74
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Enabled"=3FFF "Disabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=3FEF "UPPER-256"=3FDF "ALL"=3FCF

CHIPname=16C74A
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C74B
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C76
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C77
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C710
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000200
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FF7
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=00CF

CHIPname=16C711
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp2
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FF7
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=004F

CHIPname=16C712
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000400
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C716
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C745
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "E4 OSC"=3FFF "H4 OSC"=3FFE "EC OSC"=3FFD "HS OSC"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C765
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "E4 OSC"=3FFF "H4 OSC"=3FFE "EC OSC"=3FFD "HS OSC"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2AEF "CP75"=15DF "Enabled"=00CF

CHIPname=16C773
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "VBOR" "VBOR 25"=3FFF "VBOR 27"=3BFF "VBOR 42"=37FF "VBOR 45"=33FF
LIST4 FUSE1 "Oscillator" "RC OSC"=3FFF "HS OSC"=3FFE "XT OSC"=3FFD "LP OSC"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2EEF "CP75"=1DDF "Enabled"=0CCF

CHIPname=16C774
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=N
PowerSequence=VccVpp1
ProgramDelay=1
ProgramFlag2=25
PanelSizing=3
CoreType=bit14_A
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=Y
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "VBOR" "VBOR 25"=3FFF "VBOR 27"=3BFF "VBOR 42"=37FF "VBOR 45"=33FF
LIST4 FUSE1 "Oscillator" "RC OSC"=3FFF "HS OSC"=3FFE "XT OSC"=3FFD "LP OSC"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2EEF "CP75"=1DDF "Enabled"=0CCF

CHIPname=16C84
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Enabled"=3FFF "Disabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F54
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=7
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit12_B
ROMsize=000200
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST3 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7

CHIPname=16F57
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=7
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit12_B
ROMsize=000800
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST3 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7

CHIPname=16F59
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=7
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit12_B
ROMsize=000800
EEPROMsize=00000000
FUSEblank=0FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST3 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FF7

CHIPname=16F627
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=07A0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST6 FUSE1 "Oscillator" "ERCLK"=3FFF "ERIO"=3FFE "IRCCLK"=3FFD "IRCIO"=3FFC "EXTCLK"=3FEF "LP"=3FEC "XT"=3FED "HS"=3FEE
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2BFF "CP75"=17FF "ALL"=03FF

CHIPname=16F627A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1040
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST6 FUSE1 "Oscillator" "RCCLK"=3FFF "RCIO"=3FFE "IRCCLK"=3FFD "IRCIO"=3FFC "EXTCLK"=3FEF "LP"=3FEC "XT"=3FED "HS"=3FEE
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "ENABLED"=1FFF

CHIPname=16F628
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=07C0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST6 FUSE1 "Oscillator" "ERCLK"=3FFF "ERIO"=3FFE "IRCCLK"=3FFD "IRCIO"=3FFC "EXTCLK"=3FEF "LP"=3FEC "XT"=3FED "HS"=3FEE
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "CP50"=2BFF "CP75"=17FF "ALL"=03FF

CHIPname=16F628A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1060
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST6 FUSE1 "Oscillator" "RCCLK"=3FFF "RCIO"=3FFE "IRCCLK"=3FFD "IRCIO"=3FFC "EXTCLK"=3FEF "LP"=3FEC "XT"=3FED "HS"=3FEE
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "ENABLED"=1FFF

CHIPname=16F630
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=31FF
CPwarn=N
CALword=Y
BandGap=Y
ICSPonly=N
ChipID=10C0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Bandgap" "Highest"=3FFF "Mid High"=2FFF  "Mid Low"=1FFF "Lowest"=0FFF
LIST8 FUSE1 "Oscillator" "RC CLKGP4 RCGP5"=3FFF "RC IOGP4 RCGP5"=3FFE "INTOSC CLKGP4 IOGP5"=3FFD "INTOSC IOGP4 IOGP5"=3FFC "EC IOGP4 CLKINGP5"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F631
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1420
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC

CHIPname=16F648A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=70
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1100
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST6 FUSE1 "Oscillator" "RCCLK"=3FFF "RCIO"=3FFE "IRCCLK"=3FFD "IRCIO"=3FFC "EXTCLK"=3FEF "LP"=3FEC "XT"=3FED "HS"=3FEE
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "ENABLED"=1FFF
LIST8 FUSE1 "CPD" "Disabled"=3FFF "ENABLED"=3EFF

CHIPname=16F676
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000080
FUSEblank=31FF
CPwarn=N
CALword=Y
BandGap=Y
ICSPonly=N
ChipID=10E0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Bandgap" "Highest"=3FFF "Mid High"=2FFF  "Mid Low"=1FFF "Lowest"=0FFF
LIST8 FUSE1 "Oscillator" "RC CLKGP4 RCGP5"=3FFF "RC IOGP4 RCGP5"=3FFE "INTOSC CLKGP4 IOGP5"=3FFD "INTOSC IOGP4 IOGP5"=3FFC "EC IOGP4 CLKINGP5"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F677
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1440
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F684
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1080
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC

CHIPname=16F685
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=04A0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC

CHIPname=16F687
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1320
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC

CHIPname=16F688
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1180
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F689
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1340
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F690
INCLUDE=Y
KITSRUS.COM=14pin
EraseMode=2
FlashChip=Y
PowerSequence=Vpp2Vcc
ProgramDelay=60
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1400
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST6 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST7 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST8 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8

CHIPname=16F72
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=1
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=000800
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=00A0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F73
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=1
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0600
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F74
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=1
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0620
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F76
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=1
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0640
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F77
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=1
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0660
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST5 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FEF

CHIPname=16F737
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=3
FlashChip=Y
PowerSequence=VccFastVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0BA0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BOREN" "Enabled"=3FFF&3FFF "Sleep OFF"=3FFF&3FBF "SBOREN"=3FBF&3FFF "Disabled"=3FBF&3FBF
LIST5 FUSE1 "Brownout Voltage" "2.0V"=3FFF "2.7V"=3F7F "4.2V"=3EFF "4.5V"=3E7F
LIST6 FUSE1 "CCP2 Mux" "RC1"=3FFF "RB3"=2FFF
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF
LIST8 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST9 FUSE2 "Clock Monitor" "Enabled"=3FFF "Disabled"=3FFE
LIST10 FUSE2 "Int/Ext Switch" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F747
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=3
FlashChip=Y
PowerSequence=VccFastVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=001000
EEPROMsize=00000000
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0BE0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BOREN" "Enabled"=3FFF&3FFF "Sleep OFF"=3FFF&3FBF "SBOREN"=3FBF&3FFF "Disabled"=3FBF&3FBF
LIST5 FUSE1 "Brownout Voltage" "2.0V"=3FFF "2.7V"=3F7F "4.2V"=3EFF "4.5V"=3E7F
LIST6 FUSE1 "CCP2 Mux" "RC1"=3FFF "RB3"=2FFF
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF
LIST8 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST9 FUSE2 "Clock Monitor" "Enabled"=3FFF "Disabled"=3FFE
LIST10 FUSE2 "Int/Ext Switch" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F767
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=3
FlashChip=Y
PowerSequence=VccFastVpp1
ProgramDelay=40
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0EA0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BOREN" "Enabled"=3FFF&3FFF "Sleep OFF"=3FFF&3FBF "SBOREN"=3FBF&3FFF "Disabled"=3FBF&3FBF
LIST5 FUSE1 "Brownout Voltage" "2.0V"=3FFF "2.7V"=3F7F "4.2V"=3EFF "4.5V"=3E7F
LIST6 FUSE1 "CCP2 Mux" "RC1"=3FFF "RB3"=2FFF
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF
LIST8 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST9 FUSE2 "Clock Monitor" "Enabled"=3FFF "Disabled"=3FFE
LIST10 FUSE2 "Int/Ext Switch" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F777
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=3
FlashChip=Y
PowerSequence=VccFastVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_C
ROMsize=002000
EEPROMsize=00000000
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0DE0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BOREN" "Enabled"=3FFF&3FFF "Sleep OFF"=3FFF&3FBF "SBOREN"=3FBF&3FFF "Disabled"=3FBF&3FBF
LIST5 FUSE1 "Brownout Voltage" "2.0V"=3FFF "2.7V"=3F7F "4.2V"=3EFF "4.5V"=3E7F
LIST6 FUSE1 "CCP2 Mux" "RC1"=3FFF "RB3"=2FFF
LIST7 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF
LIST8 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST9 FUSE2 "Clock Monitor" "Enabled"=3FFF "Disabled"=3FFE
LIST10 FUSE2 "Int/Ext Switch" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F83
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=200
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000200
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=000F

CHIPname=16F84
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=200
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=FFFF
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=000F

CHIPname=16F84A
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=80
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000400
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0560
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST4 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=000F

CHIPname=16F87
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_G
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0720
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=1FFF
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST8 FUSE1 "CCPMx" "CCP1 RB0"=3FFF "CCP1 RB3"=2FFF
LIST9 FUSE1 "Debug" "Disabled"=3FFF "Enabled"=37FF
LIST10 FUSE1 "FLASH Write Protect" "Disabled"=3FFF "0000-00FF"=3DFF "0000-07FF"=3BFF "0000-0FFF"=39FF
LIST11 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST12 FUSE2 "Fail Safe" "Enabled"=3FFF "Disabled"=3FFE
LIST13 FUSE2 "Switch Over Mode" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F88
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVPP2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_G
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF 3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0760
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=1FFF
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST8 FUSE1 "CCPMx" "CCP1 RB0"=3FFF "CCP1 RB3"=2FFF
LIST9 FUSE1 "Debug" "Disabled"=3FFF "Enabled"=37FF
LIST10 FUSE1 "FLASH Write Protect" "Disabled"=3FFF "0000-00FF"=3DFF "0000-07FF"=3BFF "0000-0FFF"=39FF
LIST11 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST12 FUSE2 "Fail Safe" "Enabled"=3FFF "Disabled"=3FFE
LIST13 FUSE2 "Switch Over Mode" "Enabled"=3FFF "Disabled"=3FFD

CHIPname=16F818
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_F
ROMsize=000400
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=04C0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=1FFF
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST8 FUSE1 "CCPMx" "CCP1 RB2"=3FFF "CCP1 RB3"=2FFF
LIST9 FUSE1 "Debug" "Disabled"=3FFF "Enabled"=37FF
LIST10 FUSE1 "FLASH Write Protect" "Disabled"=3FFF "0000-01FF"=3DFF "0000-03FF"=3BFF
LIST11 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F

CHIPname=16F819
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_F
ROMsize=000800
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=04E0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "MCLRE" "Enabled"=3FFF "Disabled"=3FDF
LIST4 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST5 FUSE1 "Code Protect ROM" "Disabled"=3FFF "Enabled"=1FFF
LIST6 FUSE1 "Code Protect EEP" "Disabled"=3FFF "Enabled"=3EFF
LIST7 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EXTCLK"=3FEF "HS"=3FEE "XT"=3FED "LP"=3FEC
LIST8 FUSE1 "CCPMx" "CCP1 RB2"=3FFF "CCP1 RB3"=2FFF
LIST9 FUSE1 "Debug" "Disabled"=3FFF "Enabled"=37FF
LIST10 FUSE1 "FLASH Write Protect" "Disabled"=3FFF "0000-01FF"=3DFF "0000-03FF"=3BFF "0000-05FF"=39FF
LIST11 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F

CHIPname=16F870
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0D00
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F871
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0D20
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F872
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=000800
EEPROMsize=00000040
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=08E0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F873
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0960
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F873A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_E
ROMsize=001000
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0E40
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "WRT_256"=3DFF "WRT_1FOURTH"=3BFF "WRT_HALF"=39FF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF

CHIPname=16F874
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0920
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F874A
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_E
ROMsize=001000
EEPROMsize=00000080
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0E60
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "WRT_256"=3DFF "WRT_1FOURTH"=3BFF "WRT_HALF"=39FF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF

CHIPname=16F876
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=09E0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F876A
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_E
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0E00
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "WRT_256"=3DFF "WRT_1FOURTH"=3BFF "WRT_HALF"=39FF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF

CHIPname=16F877
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=0
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=50
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=09A0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "Disabled"=3DFF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "HALF"=2FEF "UPPER-256"=1FDF "ALL"=0FCF

CHIPname=16F877A
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=5
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=7
CoreType=bit14_E
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0E20
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FFB
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FF7
LIST3 FUSE1 "BODEN" "Enabled"=3FFF "Disabled"=3FBF
LIST4 FUSE1 "LVP" "Enabled"=3FFF "Disabled"=3F7F
LIST5 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3EFF
LIST6 FUSE1 "WRT Enable" "Enabled"=3FFF "WRT_256"=3DFF "WRT_1FOURTH"=3BFF "WRT_HALF"=39FF
LIST7 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=37FF
LIST8 FUSE1 "Oscillator" "RC"=3FFF "HS"=3FFE "XT"=3FFD "LP"=3FFC
LIST9 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=1FFF

CHIPname=16F913
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=2
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=40
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=13E0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST4 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST5 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST6 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST7 FUSE1 "MCLRE" "Disabled"=3FDF "Enabled"=3FFF
LIST8 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=2FFF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST10 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF

CHIPname=16F914
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=2
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=40
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=13C0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST4 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST5 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST6 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST7 FUSE1 "MCLRE" "Disabled"=3FDF "Enabled"=3FFF
LIST8 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=2FFF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST10 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF

CHIPname=16F916
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=2
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=40
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=13A0
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST4 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST5 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST6 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST7 FUSE1 "MCLRE" "Disabled"=3FDF "Enabled"=3FFF
LIST8 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=2FFF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST10 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF

CHIPname=16F917
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=2
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=40
ProgramFlag2=1
PanelSizing=0
CoreType=bit14_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=3FFF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1380
LIST1 FUSE1 "WDT" "Enabled"=3FFF "Disabled"=3FF7
LIST2 FUSE1 "PWRTE" "Disabled"=3FFF "Enabled"=3FEF
LIST3 FUSE1 "BODEN" "BODon SBODENoff"=3FFF "BODrun SBODENoff"=3EFF "SBODEN=PCON"=3DFF "BODoff SBODENoff"=3CFF
LIST4 FUSE1 "InEx Switch Over" "Enabled"=3FFF "Disabled"=3BFF
LIST5 FUSE1 "Fail Clock Mon" "Enabled"=3FFF "Disabled"=37FF
LIST6 FUSE1 "CPD" "Disabled"=3FFF "Enabled"=3F7F
LIST7 FUSE1 "MCLRE" "Disabled"=3FDF "Enabled"=3FFF
LIST8 FUSE1 "DEBUG" "Disabled"=3FFF "Enabled"=2FFF
LIST9 FUSE1 "Oscillator" "EXTRC_CLKOUT"=3FFF "EXTRC_IO"=3FFE "INTRC_CLKOUT"=3FFD "INTRC_IO"=3FFC "EC"=3FFB "HS"=3FFA "XT"=3FF9 "LP"=3FF8
LIST10 FUSE1 "Code Protect" "Disabled"=3FFF "Enabled"=3FBF

CHIPname=18F242
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0480
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST9 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST10 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST11 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST12 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST13 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST14 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST15 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST16 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST17 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST18 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST19 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST21 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST23 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F248
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0800
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST9 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST10 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST11 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST12 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST13 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST14 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST15 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST17 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST18 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST19 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST20 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F252
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0400
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST9 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST10 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST11 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST12 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST13 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST14 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST15 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST16 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST17 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST18 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST19 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST20 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST28 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST29 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F258
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0840
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST9 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST10 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST11 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST12 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST13 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST14 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST15 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST16 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST17 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST19 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST21 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST22 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST24 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST25 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST26 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F442
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=04A0
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST9 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST10 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST11 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST12 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST13 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST14 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST15 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST16 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST17 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST18 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST19 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST21 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST23 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F448
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0820
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST9 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST10 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST11 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST12 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST13 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST14 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST15 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST17 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST18 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST19 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST20 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F452
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0420
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST9 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST10 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST11 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST12 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST13 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST14 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST15 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST16 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST17 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST18 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST19 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST20 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST28 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST29 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F458
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0100 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0860
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST9 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST10 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST11 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST12 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST13 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST14 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST15 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST16 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST17 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST19 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST21 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST22 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST24 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST25 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST26 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F1220
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8000 0085 C003 E003 4003
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=07E0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST11 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST12 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST13 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST14 FUSE5 "ROM Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST15 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST16 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST17 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE6 "ROM Table Write Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST19 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST20 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST22 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST23 FUSE7 "ROM Table Read Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST24 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD

CHIPname=18F1320
INCLUDE=Y
KITSRUS.COM=18pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp2
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8000 0085 C003 E003 4003
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=07C0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST11 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST12 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST13 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST14 FUSE5 "ROM Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST15 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST16 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST17 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE6 "ROM Table Write Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST19 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST20 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST22 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST23 FUSE7 "ROM Table Read Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST24 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD

CHIPname=18F2220
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8300 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0580
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "1000-17FF Disabled"=FFFF "1000-5FFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "1800-1FFF Disabled"=FFFF "1800-7FFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7

CHIPname=18F2221
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2160
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "BBSIZ" "512 words"=FFFF "256 words"=FCFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST19 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST21 FUSE6 "ROM Table Write Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST22 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD

CHIPname=18F2320
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8300 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0500
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "1000-17FF Disabled"=FFFF "1000-5FFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "1800-1FFF Disabled"=FFFF "1800-7FFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7

CHIPname=18F2321
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2120
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "BBSIZ" "1K words"=FFFF "512 words"=FDFF "256 words"=FCFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST19 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST21 FUSE6 "ROM Table Write Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST22 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD

CHIPname=18F2331
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 3F0F 9D3C 0085 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=08E0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE2 "Winen" "Enabled"=FFFF "Disabled"=FDFF
LIST10 FUSE3 "GPTREN" "Disabled"=FFFF "Enabled"=FFDF
LIST11 FUSE3 "HPOL" "Active High"=FFFF "Active Low"=FFEF
LIST12 FUSE3 "LPOL" "Active High"=FFFF "Active Low"=FFF7
LIST13 FUSE3 "PWMPIN" "Disabled"=FFFF "Enabled"=FFFB
LIST14 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST15 FUSE3 "EXCLKMX" "MUX with RC3"=FFFF "MUX with RD0"=EFFF
LIST16 FUSE3 "PWM4MX" "Enabled"=FFFF "Disabled"=FDFF
LIST17 FUSE3 "SSPMX" "MUX RC5,RC4,RC7"=FFFF "MUX RD3,RD2,RD1"=FBFF
LIST18 FUSE3 "FLTAMX" "MUX with RC1"=FFFF "MUX with RD4"=FEFF
LIST19 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST20 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST21 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE5 "ROM Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST23 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST24 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE6 "ROM Table Write Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST27 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD

CHIPname=18F2410
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000000
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1160
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST21 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST22 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST23 FUSE6 "ROM Table Write Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST24 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST25 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST27 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST28 FUSE7 "ROM Table Read Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST29 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD

CHIPname=18F2420
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0C80
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST21 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST22 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST23 FUSE6 "ROM Table Write Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST24 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST25 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST27 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST28 FUSE7 "ROM Table Read Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST29 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD

CHIPname=18F2431
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 3F0F 9D3C 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=08C0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE2 "Winen" "Enabled"=FFFF "Disabled"=FDFF
LIST10 FUSE3 "GPTREN" "Disabled"=FFFF "Enabled"=FFDF
LIST11 FUSE3 "HPOL" "Active High"=FFFF "Active Low"=FFEF
LIST12 FUSE3 "LPOL" "Active High"=FFFF "Active Low"=FFF7
LIST13 FUSE3 "PWMPIN" "Disabled"=FFFF "Enabled"=FFFB
LIST14 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST20 FUSE5 "ROM Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST21 FUSE5 "ROM Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7
LIST22 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST24 FUSE6 "ROM Table Write Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST25 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST26 FUSE6 "ROM Table Write Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST27 FUSE6 "ROM Table Write Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST33 FUSE7 "ROM Table Read Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST34 FUSE7 "ROM Table Read Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7

CHIPname=18F2450
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000000
FUSEblank=CF3F 1F3F 8700 00E5 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2420
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FF7F
LIST18 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST19 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST20 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST21 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST22 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST23 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST24 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST25 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST27 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST28 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST29 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST30 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST31 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST32 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST33 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST34 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2455
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=003000
EEPROMsize=00000100
FUSEblank=CF3F 1F3F 8700 00E5 C007 E007 4007 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1260
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST18 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST19 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST20 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST23 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST24 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST27 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST28 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2480
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8600 00D5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1AE0
LIST1 FUSE1 "Osc Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.1V"=FFFF "2.8V"=FFF7 "4.3V"=FFFD "4.6V"=FFF9
LIST5 FUSE2 "Brownout Reset" "HW only"=FFFF "HW but not sleep"=FFFB "Enabled under SW ctrl"=FFFD "Disabled"=FFF0
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST12 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST24 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST26 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST27 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST28 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2510
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000000
FUSEblank=CF00 1F1F 8700 00C5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1120
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST25 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST26 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2520
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0C80
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST25 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST26 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2550
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=05
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF3F 1F3F 8700 00E5 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1240
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST18 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST19 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST20 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST23 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST24 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST25 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST27 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST28 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST29 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST30 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST31 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST32 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST33 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST34 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F2580
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8600 00D5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1AC0
LIST1 FUSE1 "Osc Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.1V"=FFFF "2.8V"=FFF7 "4.3V"=FFFD "4.6V"=FFF9
LIST5 FUSE2 "Brownout Reset" "HW only"=FFFF "HW but not sleep"=FFFB "Enabled under SW ctrl"=FFFD "Disabled"=FFF0
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST12 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-0BBSIZ Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST21 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST22 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST24 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST25 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST26 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST27 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST33 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST34 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F4220
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8300 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=05A0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "1000-17FF Disabled"=FFFF "1000-5FFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "1800-1FFF Disabled"=FFFF "1800-7FFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7

CHIPname=18F4221
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=000800
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8300 0085 C003 E003 4003
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2140
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "BBSIZ" "512 words"=FFFF "256 words"=FCFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST19 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST21 FUSE6 "ROM Table Write Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST22 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "BBSIZ-07FF Disabled"=FFFF "BBSIZ-07FF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD

CHIPname=18F4320
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 1F0F 8300 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0520
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "1000-17FF Disabled"=FFFF "1000-5FFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "1800-1FFF Disabled"=FFFF "1800-7FFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0200-07FF Disabled"=FFFF "0200-07FF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "0800-0FFF Disabled"=FFFF "0800-0FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "1000-17FF Disabled"=FFFF "1000-17FF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "1800-1FFF Disabled"=FFFF "1800-1FFF Enabled"=FFF7

CHIPname=18F4321
INCLUDE=Y
KITSRUS.COM=28Npin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2100
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST10 FUSE3 "PORTB AD Enable" "Enabled"=FFFF "Disabled"=FDFF
LIST11 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST12 FUSE4 "BBSIZ" "1K words"=FFFF "512 words"=FDFF "256 words"=FCFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST19 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST21 FUSE6 "ROM Table Write Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST22 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "BBSIZ-0FFF Disabled"=FFFF "BBSIZ-0FFF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD

CHIPname=18F4331
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=001000
EEPROMsize=00000100
FUSEblank=CF00 3F0F 9D3C 0085 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=08A0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE2 "Winen" "Enabled"=FFFF "Disabled"=FDFF
LIST10 FUSE3 "GPTREN" "Disabled"=FFFF "Enabled"=FFDF
LIST11 FUSE3 "HPOL" "Active High"=FFFF "Active Low"=FFEF
LIST12 FUSE3 "LPOL" "Active High"=FFFF "Active Low"=FFF7
LIST13 FUSE3 "PWMPIN" "Disabled"=FFFF "Enabled"=FFFB
LIST14 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST15 FUSE3 "EXCLKMX" "MUX with RC3"=FFFF "MUX with RD0"=EFFF
LIST16 FUSE3 "PWM4MX" "Enabled"=FFFF "Disabled"=FDFF
LIST17 FUSE3 "SSPMX" "MUX RC5,RC4,RC7"=FFFF "MUX RD3,RD2,RD1"=FBFF
LIST18 FUSE3 "FLTAMX" "MUX with RC1"=FFFF "MUX with RD4"=FEFF
LIST19 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST20 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST21 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE5 "ROM Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST23 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST24 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE6 "ROM Table Write Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST27 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD

CHIPname=18F4410
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000000
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=10E0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST21 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST22 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST23 FUSE6 "ROM Table Write Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST24 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST25 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST27 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST28 FUSE7 "ROM Table Read Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST29 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD

CHIPname=18F4420
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C003 E003 4003
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0C80
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST21 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST22 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST23 FUSE6 "ROM Table Write Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST24 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST25 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST27 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST28 FUSE7 "ROM Table Read Protect" "BBSIZ-3FFF Disabled"=FFFF "BBSIZ-3FFF Enabled"=FFFE
LIST29 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD

CHIPname=18F4431
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 3F0F 9D3C 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=0880
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "ExRC OSC1 CO OSC2"=FFFF "IRC O1RA7 CO OSC2"=F9FF "IRC O1RA7 O2RA6"=F8FF "ExRC OSC2 RA6"=F7FF "HS+PLL"=F6FF "ExOSC1 CO RA6"=F5FF "ExOSC1 CO OSC2"=F4FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FEFF "1:8192"=FDFF "1:4096"=FCFF "1:2048"=FBFF "1:1024"=FAFF "1:512"=F9FF "1:256"=F8FF "1:128"=F7FF "1:64"=F6FF "1:32"=F5FF "1:16"=F4FF "1:8"=F3FF "1:4"=F2FF "1:2"=F1FF "1:1"=F0FF
LIST9 FUSE2 "Winen" "Enabled"=FFFF "Disabled"=FDFF
LIST10 FUSE3 "GPTREN" "Disabled"=FFFF "Enabled"=FFDF
LIST11 FUSE3 "HPOL" "Active High"=FFFF "Active Low"=FFEF
LIST12 FUSE3 "LPOL" "Active High"=FFFF "Active Low"=FFF7
LIST13 FUSE3 "PWMPIN" "Disabled"=FFFF "Enabled"=FFFB
LIST14 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST20 FUSE5 "ROM Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST21 FUSE5 "ROM Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7
LIST22 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST24 FUSE6 "ROM Table Write Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST25 FUSE6 "ROM Table Write Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST26 FUSE6 "ROM Table Write Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST27 FUSE6 "ROM Table Write Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "0200-0FFF Disabled"=FFFF "0200-0FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "1000-1FFF Disabled"=FFFF "1000-1FFF Enabled"=FFFD
LIST33 FUSE7 "ROM Table Read Protect" "2000-2FFF Disabled"=FFFF "2000-2FFF Enabled"=FFFB
LIST34 FUSE7 "ROM Table Read Protect" "3000-3FFF Disabled"=FFFF "3000-3FFF Enabled"=FFF7

CHIPname=18F4450
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000000
FUSEblank=CF3F 1F3F 8700 00E5 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=2400
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FF7F
LIST18 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST19 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST20 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST21 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST22 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST23 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST24 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST25 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST27 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST28 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST29 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST30 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST31 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST32 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST33 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST34 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4455
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=003000
EEPROMsize=00000100
FUSEblank=CF3F 1F3F 8700 00E5 C007 E007 4007 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1220
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST18 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST19 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST20 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST23 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST24 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST27 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST28 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4480
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=002000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8600 00D5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1AA0
LIST1 FUSE1 "Osc Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.1V"=FFFF "2.8V"=FFF7 "4.3V"=FFFD "4.6V"=FFF9
LIST5 FUSE2 "Brownout Reset" "HW only"=FFFF "HW but not sleep"=FFFB "Enabled under SW ctrl"=FFFD "Disabled"=FFF0
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST12 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST24 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST26 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST27 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST28 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4510
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000000
FUSEblank=CF00 1F1F 8700 00C5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=10A0
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST25 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST26 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4520
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8700 00C5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1080
LIST1 FUSE1 "IE Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail Safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST5 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "HighPower Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Analog on Reset"=FFFF "AD 4:0 Digital on Reset"=FDFF
LIST12 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST13 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST14 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST15 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST16 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST17 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST18 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST19 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST20 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST25 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST26 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST27 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST28 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST29 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST30 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST31 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST32 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST33 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4550
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=05
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF3F 1F3F 8700 00E5 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1200
LIST1 FUSE1 "USBPLL" "Divide by 2"=FFFF "No Divide"=FFDF
LIST2 FUSE1 "CPUDIV" "Div/6 wPLL, Div/4"=FFFF "Div/4 wPLL, Div/3"=FFF7 "Div/3 wPLL, Div/2"=FFEF "Div/2 wPLL, NO Div"=FFE7
LIST3 FUSE1 "PPLDIV" "Osc/12 (48Mhz)"=FFFF "Osc/10 (40Mhz)"=FFFE "Osc/6 (24Mhz)"=FFFD "Osc/5 (20Mhz)"=FFFC "Osc/4 (16Mhz)"=FFFB "Osc/3 (12Mhz)"=FFFA "Osc/2 (8Mhz)"=FFF9 "No Divide (4Mhz)"=FFF8
LIST4 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST5 FUSE1 "Oscillator" "HS OSC w/PLL, HS used by USB"=FFFF "HS osc, HS used by USB"=FCFF "Intrn osc, HS used by USB"=FBFF "Intrn osc, XT used by USB"=FAFF
LIST6 FUSE2 "VREGEN" "Enabled"=FFFF "Disabled"=FFFD
LIST7 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST8 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST9 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST10 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST12 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST13 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST14 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST15 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST16 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST17 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST18 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST19 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST20 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST21 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST22 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST23 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST24 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST25 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST27 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST28 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST29 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST30 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST31 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST32 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST33 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST34 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD

CHIPname=18F4580
INCLUDE=Y
KITSRUS.COM=40pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=CF00 1F1F 8600 00D5 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=N
ChipID=1A80
LIST1 FUSE1 "Osc Switchover" "Enabled"=FFFF "Disabled"=7FFF
LIST2 FUSE1 "Fail safe Clock Mon" "Enabled"=FFFF "Disabled"=BFFF
LIST3 FUSE1 "Oscillator" "LP Osc"=F0FF "XT Osc"=F1FF "HS Osc"=F2FF "Ext RC"=F3FF "EC Osc"=F4FF "EC Port RA6"=F5FF "HSPLL"=F6FF "Ext RC"=F7FF "Int OSC"=F8FF "Int OSC Clk RA6 PortB"=F9FF "Int Osc Clk RA6"=FBFF "Int Osc Clk RA6"=FCFF
LIST4 FUSE2 "Brownout Voltage" "2.1V"=FFFF "2.8V"=FFF7 "4.3V"=FFFD "4.6V"=FFF9
LIST5 FUSE2 "Brownout Reset" "HW only"=FFFF "HW but not sleep"=FFFB "Enabled under SW ctrl"=FFFD "Disabled"=FFF0
LIST6 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST9 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST10 FUSE3 "LPT1OSC" "LOW Power Mode"=FFFF "High Pwr Mode"=FBFF
LIST11 FUSE3 "PBADEN" "AD 4:0 Reset=Analog"=FFFF "AD 4:0 Reset=Digital"=FDFF
LIST12 FUSE4 "BBSIZ" "2K words"=FFFF "1K words"=FEFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "XINST" "Enabled"=FFFF "Disabled"=FFBF
LIST15 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST16 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST17 FUSE5 "BOOT ROM Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST18 FUSE5 "ROM Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST19 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST20 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST21 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST22 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST23 FUSE6 "BOOT Table Write Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST24 FUSE6 "ROM Table Write Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST25 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST26 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST27 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST28 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST29 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST30 FUSE7 "BOOT Table Read Protect" "0000-BBSIZ Disabled"=FFFF "0000-BBSIZ Enabled"=BFFF
LIST31 FUSE7 "ROM Table Read Protect" "BBSIZ-1FFF Disabled"=FFFF "BBSIZ-1FFF Enabled"=FFFE
LIST32 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST33 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST34 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F6520
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0383 0085 C00F E00F 400F 
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0B20
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST9 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST10 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST11 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST12 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST13 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST14 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST15 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST16 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST17 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST18 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST19 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST20 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST21 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST22 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST23 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST24 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST25 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST26 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST27 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST28 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST29 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F6525
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_C
ROMsize=006000
EEPROMsize=00000100
FUSEblank=2F00 1F0F 8383 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0AE0
LIST1 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RC OSC2 RA6"=FFFF "HS PLL"=FEFF "EC OSC2RA6"=FDFF "EC OSC2RA6 PLL"= FCFF "RC OSC2RA6"=F7FF "HS PLL"=F6FF "EC OSC2RA6"=F5FF "EC OSC2/4"=F4FF "RC OSC2/4"=F3FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST7 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST8 FUSE3 "WAIT" "Disabled"=FFFF "MEMCON"=FF7F
LIST9 FUSE3 "Processor Mode" "Microcontroller"=FFFF "Microprocessor"=FFFE "Microprocessor Boot"=FFFD "Extended"=FFFC
LIST10 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST11 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST19 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST20 FUSE6 "BOOT Table Write Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST21 FUSE6 "ROM Table Write Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST22 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST23 FUSE6 "ROM Table Write Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST24 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST25 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST26 FUSE7 "BOOT Table Read Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST27 FUSE7 "ROM Table Read Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST28 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST29 FUSE7 "ROM Table Read Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB

CHIPname=18F6621
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_C
ROMsize=008000
EEPROMsize=00000100
FUSEblank=2F00 1F0F 8383 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0AA0
LIST1 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RC OSC2 RA6"=FFFF "HS PLL"=FEFF "EC OSC2RA6"=FDFF "EC OSC2RA6 PLL"= FCFF "RC OSC2RA6"=F7FF "HS PLL"=F6FF "EC OSC2RA6"=F5FF "EC OSC2/4"=F4FF "RC OSC2/4"=F3FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST7 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST8 FUSE3 "WAIT" "Disabled"=FFFF "MEMCON"=FF7F
LIST9 FUSE3 "Processor Mode" "Microcontroller"=FFFF "Microprocessor"=FFFE "Microprocessor Boot"=FFFD "Extended"=FFFC
LIST10 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST11 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "C000-FFFF Disabled"=FFFF "C000-7FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "C000-FFFF Disabled"=FFFF "C000-FFFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "C000-FFFF Disabled"=FFFF "C000-FFFF Enabled"=FFF7

CHIPname=18F8520
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=004000
EEPROMsize=00000100
FUSEblank=2700 0F0F 0383 0085 C0FF E0FF 40FF
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0B00
LIST1 FUSE1 "Oscillator Enable" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RCO2RA6"=FFFF "HSPLL"=FEFF "ECO2RA6"=FDFF "ECO2 CLK Out"=FCFF "RC"=FBFF "HS"=FAFF "XT"=F9FF "LP"=F8FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Postscale" "1:128"=FFFF "1:64"=FDFF "1:32"=FBFF "1:16"=F9FF "1:8"=F7FF "1:4"=F5FF "1:2"=F3FF "1:1"=F1FF
LIST7 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST8 FUSE3 "WAIT" "Disabled"=FFFF "MEMCON"=FF7F
LIST9 FUSE3 "T1OSCMX" "Legacy Timer1"=FFFF "Low Power"=FDFF
LIST10 FUSE3 "CCP2 Mux" "Enabled"=FFFF "Disabled"=FEFF
LIST11 FUSE3 "PM1:0" "MicroController"=FFFF "Microprocessor"=FFFE "uProcessor with Boot"=FFFD "Extend uProcessor"=FFFC
LIST12 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST13 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST14 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST15 FUSE5 "BOOT ROM Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST16 FUSE5 "ROM Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST17 FUSE5 "ROM Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST18 FUSE5 "ROM Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST19 FUSE5 "ROM Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST25 FUSE6 "ROM Table Write Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7
LIST26 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST27 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST28 FUSE7 "BOOT Table Read Protect" "0000-01FF Disabled"=FFFF "0000-01FF Enabled"=BFFF
LIST29 FUSE7 "ROM Table Read Protect" "0200-1FFF Disabled"=FFFF "0200-1FFF Enabled"=FFFE
LIST30 FUSE7 "ROM Table Read Protect" "2000-3FFF Disabled"=FFFF "2000-3FFF Enabled"=FFFD
LIST31 FUSE7 "ROM Table Read Protect" "4000-5FFF Disabled"=FFFF "4000-5FFF Enabled"=FFFB
LIST32 FUSE7 "ROM Table Read Protect" "6000-7FFF Disabled"=FFFF "6000-7FFF Enabled"=FFF7

CHIPname=18F8525
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_C
ROMsize=006000
EEPROMsize=00000100
FUSEblank=2F00 1F0F 8383 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0AC0
LIST1 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RC OSC2 RA6"=FFFF "HS PLL"=FEFF "EC OSC2RA6"=FDFF "EC OSC2RA6 PLL"= FCFF "RC OSC2RA6"=F7FF "HS PLL"=F6FF "EC OSC2RA6"=F5FF "EC OSC2/4"=F4FF "RC OSC2/4"=F3FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST7 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST8 FUSE3 "WAIT" "Disabled"=FFFF "MEMCON"=FF7F
LIST9 FUSE3 "Processor Mode" "Microcontroller"=FFFF "Microprocessor"=FFFE "Microprocessor Boot"=FFFD "Extended"=FFFC
LIST10 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST11 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST12 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST19 FUSE5 "ROM Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST20 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST21 FUSE6 "BOOT Table Write Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST22 FUSE6 "ROM Table Write Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST23 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST24 FUSE6 "ROM Table Write Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST25 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST26 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST27 FUSE7 "BOOT Table Read Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST28 FUSE7 "ROM Table Read Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST29 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST30 FUSE7 "ROM Table Read Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB

CHIPname=18F8621
INCLUDE=Y
KITSRUS.COM=0pin
EraseMode=4
FlashChip=Y
PowerSequence=VccVpp1
ProgramDelay=10
ProgramFlag2=1
PanelSizing=0
CoreType=bit16_B
ROMsize=008000
EEPROMsize=00000100
FUSEblank=2F00 1F0F 8383 0085 C00F E00F 400F
CPwarn=N
CALword=N
BandGap=N
ICSPonly=Y
ChipID=0A80
LIST1 FUSE1 "OSCSEN" "Disabled"=FFFF "Enabled"=DFFF
LIST2 FUSE1 "Oscillator" "RC OSC2 RA6"=FFFF "HS PLL"=FEFF "EC OSC2RA6"=FDFF "EC OSC2RA6 PLL"= FCFF "RC OSC2RA6"=F7FF "HS PLL"=F6FF "EC OSC2RA6"=F5FF "EC OSC2/4"=F4FF "RC OSC2/4"=F3FF "HS"=F2FF "XT"=F1FF "LP"=F0FF
LIST3 FUSE2 "Brownout Voltage" "2.0V"=FFFF "2.7V"=FFFB "4.2V"=FFF7 "4.5V"=FFF3
LIST4 FUSE2 "Brownout Detect" "Enabled"=FFFF "Disabled"=FFFD
LIST5 FUSE2 "Powerup Timer" "Disabled"=FFFF "Enabled"=FFFE
LIST6 FUSE2 "Watchdog Timer" "Enabled"=FFFF "Disabled"=FEFF
LIST7 FUSE2 "Watchdog Postscale" "1:32768"=FFFF "1:16384"=FDFF "1:8192"=FBFF "1:4096"=F9FF "1:2048"=F7FF "1:1024"=F5FF "1:512"=F3FF "1:256"=F1FF "1:128"=EFFF "1:64"=EDFF "1:32"=EBFF "1:16"=E9FF "1:8"=E7FF "1:4"=E5FF "1:2"=E3FF "1:1"=E1FF
LIST8 FUSE3 "WAIT" "Disabled"=FFFF "MEMCON"=FF7F
LIST9 FUSE3 "Processor Mode" "Microcontroller"=FFFF "Microprocessor"=FFFE "Microprocessor Boot"=FFFD "Extended"=FFFC
LIST10 FUSE3 "MCLRE" "Enabled"=FFFF "Disabled"=7FFF
LIST11 FUSE3 "CCP2MX" "MUC RC1"=FFFF "MUC RE7/RB3"=FEFF
LIST12 FUSE3 "ECCMUX" "ENH CCP1 RE6 3"=FFFF "ENH CCP1 RH7 4"=FDFF
LIST13 FUSE4 "Background Debug" "Disabled"=FFFF "Enabled"=FF7F
LIST14 FUSE4 "Low Voltage Program" "Enabled"=FFFF "Disabled"=FFFB
LIST15 FUSE4 "Stack Overflow Reset" "Enabled"=FFFF "Disabled"=FFFE
LIST16 FUSE5 "BOOT ROM Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST17 FUSE5 "ROM Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST18 FUSE5 "ROM Protect" "0400-7FFF Disabled"=FFFF "0400-7FFF Enabled"=FFFD
LIST19 FUSE5 "ROM Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST20 FUSE5 "ROM Protect" "C000-FFFF Disabled"=FFFF "C000-7FFF Enabled"=FFF7
LIST21 FUSE5 "EEPROM Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST22 FUSE6 "BOOT Table Write Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST23 FUSE6 "ROM Table Write Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST24 FUSE6 "ROM Table Write Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST25 FUSE6 "ROM Table Write Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST26 FUSE6 "ROM Table Write Protect" "C000-FFFF Disabled"=FFFF "C000-FFFF Enabled"=FFF7
LIST27 FUSE6 "EEPROM Table Write Protect" "Disabled"=FFFF "Enabled"=7FFF
LIST28 FUSE6 "CONFIG Table Write Protect" "Disabled"=FFFF "Enabled"=DFFF
LIST29 FUSE7 "BOOT Table Read Protect" "0000-07FF Disabled"=FFFF "0000-07FF Enabled"=BFFF
LIST30 FUSE7 "ROM Table Read Protect" "0800-3FFF Disabled"=FFFF "0800-3FFF Enabled"=FFFE
LIST31 FUSE7 "ROM Table Read Protect" "4000-7FFF Disabled"=FFFF "4000-7FFF Enabled"=FFFD
LIST32 FUSE7 "ROM Table Read Protect" "8000-BFFF Disabled"=FFFF "8000-BFFF Enabled"=FFFB
LIST33 FUSE7 "ROM Table Read Protect" "C000-FFFF Disabled"=FFFF "C000-FFFF Enabled"=FFF7